280595 Serial Commands

|  |  |
| --- | --- |
| Baud Rate : | 115200 bps |
| Data Bit : | 8 bits |
| Parity : | None |
| Stop Bit : | 1 bit |



\***PLEASE NOTE THAT A CARRIAGE RETURN IS REQUIRED AFTER EACH COMMAND IS SENT.**



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ASCII Command | Action | Response | Example | Description |
| I?? | ??:Source number 0~ 12 input source 00: for close output 01: for CVBS 1 02: for CVBS 2 03: for S-video 1 04: for S-video 2 05: for Ypbpr 1 06: for Ypbpr 2 07: for VGA 08: for DVI 09: for HDMI 1 10: for HDMI 2 11: for HDMI 3 12: for HDMI 4 | i?? | >>I02 i02 >>I00 i00 | Select source 02 (CVBS2)  Close output |