280595 Serial Commands

|  |  |
| --- | --- |
|  Baud Rate : | 115200 bps |
| Data Bit : | 8 bits |
| Parity : | None |
| Stop Bit : | 1 bit |

\***PLEASE NOTE THAT A CARRIAGE RETURN IS REQUIRED AFTER EACH COMMAND IS SENT.**



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ASCII Command | Action | Response | Example | Description |
| I?? | ??:Source number 0~ 12 input source00: for close output01: for CVBS 102: for CVBS 203: for S-video 104: for S-video 205: for Ypbpr 106: for Ypbpr 207: for VGA08: for DVI09: for HDMI 110: for HDMI 211: for HDMI 312: for HDMI 4 | i?? | >>I02i02>>I00i00 | Select source 02 (CVBS2)Close output |